# USB Device Operational Settings

This page explains the operational settings that can be configured for each USB device connected to a device server.

1. Change the USB device name displayed in SX Virtual Link's main window

2. Automatically connect to a USB device when it is detected

3. Automatically reconnect to a USB device when it is disconnected abnormally

4. Automatically start a designated application when a USB device is connected

5. Automatically disconnect from a USB device when a disconnect request is received

6. About the USB device properties dialog

## 1.Change the USB device name displayed in SX Virtual Link's main window

In SX Virtual Link's main window, the default name originally registered to the USB device is shown in the USB device list.

The USB device name can be changed from the General tab in the properties dialog.
For details on the properties dialog, refer to 6. About the USB device properties dialog.

Even if the device name is changed, the default name originally registered to the device is not changed. Also, this change takes effect only for the PC from which you have changed the device name and not for other PCs.

## 2. Automatically connect to a USB device when it is detected

SX Virtual Link can automatically connect to a USB device when it is detected.
If you are the only person that will use a particular USB device, you can utilize the auto-connect function to automatically connect to the USB device without clicking the Connect button on SX Virtual Link's main window.

The auto-connect function can be enabled from the Connect tab in the properties dialog.
For details on the properties dialog, refer to 6. About the USB device properties dialog.

If you wish to connect to all USB devices automatically, check the Automatically connect newly discovered USB devices check box on the SX Virtual Link option dialog. For details, refer to SX Virtual Link Optional Settings.

## 3. Automatically reconnect to a USB device when it is disconnected abnormally

SX Virtual Link can automatically reconnect to a USB device when the connection between the USB device and your PC is lost due to a communication error.

The auto-reconnect option for USB devices that have been abnormally disconnected can be enabled from the Connect tab in the properties dialog.
For details on the properties dialog, refer to 6. About the USB device properties dialog.

The auto-reconnect setting will take effect the next time you connect to the USB device.

The auto-reconnect feature may not work properly depending on the USB device or PC's status during the error. In such a case, reboot the PC, USB device and device server. This option is only for recovery purposes in case of an error. Please do not unplug the USB device intentionally while it is connected to your PC via SX Virtual Link.

## 4. Automatically start a designated application when a USB device is connected

SX Virtual Link can automatically start a designated application when a USB device is connected to your PC.
The auto-application startup feature can be enabled by registering the application that you wish to use with a particular USB device (e.g. image reading software for a scanner, music management software for a music player, backup software for storage media, etc) to SX Virtual Link. After an application is registered to SX Virtual Link, it will automatically start when the USB device is connected to your PC via SX Virtual Link. Thus, you will not have to manually start the application.

The auto-application startup feature can be enabled from the Connect tab in the properties dialog.
For details on the properties dialog, refer to 6. About the USB device properties dialog.

The auto-application startup feature will take effect the next time you connect to the USB device.

## 5. Automatically disconnect from a USB device when a disconnect request is received

SX Virtual Link can automatically disconnect from a USB device when a disconnect request is received.

The auto-disconnect setting can be enabled from the Disconnect tab in the properties dialog.
For details on the properties dialog, refer to 6. About the USB device properties dialog.

## 6. About the USB device properties dialog

The above operational settings are available from the properties dialog of each USB device.

How to open and use the properties dialog:

1. Select the USB device in SX Virtual Link's main window and click the Properties button .

2. The General tab is displayed. In the General tab, you can change the USB device name to be displayed in SX Virtual Link's main window.

   Name | Change the USB device name to be displayed in SX Virtual Link's main window. For details, refer to 1. Change the USB device name displayed in SX Virtual Link's main window.
   Device Server Properties | Opens the Web page of the device server. On the Web page, various settings are available. For details, please refer to the users manual.

3. If you click the Connect tab, you can configure the settings shown below.

   Automatically connect this device when it is available | Automatically connects on detection of a USB device with this option enabled. For details, refer to 2. Automatically connect to a USB device when it is detected.
   If an error occurs while connected, automatically reconnect | Automatically reconnects to a USB device when it is disconnected from the PC due to a communication error. For details, refer to 3. Automatically reconnect to a USB device when it is disconnected abnormally.
   Start designated application when connected | Automatically starts a designated application when the USB device is connected to your PC via SX Virtual Link. Also, if you check the Disconnect automatically when application is closed check box, the USB device will be automatically disconnected when the application is closed. For details, refer to 4. Automatically start a designated application when the USB device is connected.

4. If you click the Disconnect tab, you can configure the auto-disconnect settings.

   Allow auto-disconnect when a Request Use is received | Automatically disconnects from a USB device when a disconnect request is received. For details, refer to 5. Automatically disconnect from a USB device when a disconnect request is received. * If this option is enabled, the USB device will be disconnected even if it is being used when the Request Use is received. * To allow your PC to immediately disconnect from a USB device if a Request Use is received when a lock screen is displayed, check the Always accept a Request Use when a lock screen is displayed check box on the SX Virtual Link option dialog. For details, refer to SX Virtual Link Optional Settings.
   Auto-disconnect timeout | Waits a specified amount of time before disconnecting a USB device when Allow auto-disconnect when a Request Use is received is enabled.

5. If you click the Security tab, you can configure the security settings to use the USB device.

   Specify the USB connection password | Set the password to be entered when the USB device is connected. If this setting is enabled, the password will automatically be entered when the USB device is connected. When the device server does not support the USB connection password feature, this field is grayed out.
   Password | Enter the password. When the device server does not support the USB connection password feature, this field is grayed out.
   Enable data encryption for USB device | Enables encryption for USB device communication. When the device server does not support the encryption, this field is grayed out.

   The Security tab is displayed only when the device server supports the USB connection password and encryption. If these features are not supported, the corresponding settings will be grayed out.

6. When configuration is complete, click OK.

| Back to Top