[FIRMWARE]
Product=SX-590
Version=1.30
MD5=cc5dd72eac196d4042b7a074bec61545
SHA1=6a48cffeebccd557ca16e2bc5ed11f778a9dd3a8

RELEASE NOTES:
Ver. 1.00 
•	Initial Release.

Version 1.01 
•	Fixed error in background scanning behavior that was happening while data reception
was consecutively occurring using UDP.
•	Fixed a problem that was causing speed to drastically slow down as the transmitting data was
dropped into AP mode.
•	Fixed WPA2 vulnerability issue (KRACK).
•	Fixed an unexpected behavior in AMC Manager taking a long time to find a device. 
•	Fixed a communication error that occurred when WEP key Index was different from
the one used for the access point.

Ver. 1.02
•	Fixed an error in the wireless data transmission randomly stacking up and then
slowing down in speed while data reception was consecutively occurring using TCP.
•	Fixed an error that prevented the SH NW WLLIST command from showing an effective channel
number.
•	Fixed an error that prevented the SH NW WLLIST command from recognizing 11n and 11ac.
•	Fixed vulnerability in HTTP POST command injection.
•	Supported R&TTE Adaptivity.
•	Supported a region code for WWR.

Ver. 1.03
•	Supported RED (EN301893 V2.1.1).

Ver. 1.04
•	Enhanced security functions.
•	Supported RE Directives.
Ver. 1.10
•	  Fixed bug that occurred because the IP address was not set by BOOTP.
•	  Fixed command injection vulnerability in NTP server setting.
•	  Corrected WEB page display defects occurring after Edge 42 or later.
•	  Improved stability of multi-client bridge that corresponds with Canadian (CA) destination    
  setting.
•	  Supported auto-detection of country code in WWR mode.
•	  Enhanced WEB page security.
i.	Made HTTPS compliant.
ii.	Added login control (response to Brute Force Attack).
iii.	Response to Cross Site Scripting (XSS).
•	  Security extension correspondence.
•	  Made TCP port and E-cable mode TSL compatible.
•	  Added power saving support.
•	  Added SSH support.

Ver 1.11
•	Fixed minor bugs.

Ver. 1.20
•	Fixed minor bugs.
•	Added and updated functions: 
i.	Added DFS band channel support in AP mode.
ii.	Updated Openssl version to Ver.1.1.1.
iii.	Supported TLS 1.2 (*) for enterprise authentication. 
iv.	Added IEEE 802.11r function.
v.	Added the user ID anonymous function for EAP authentication.
* Note: When TLS 1.2 is in use, the certificate with the key size of at least 1024 bits or more needs to be          
  used. It is recommended to use 2048 bit or greater keys for security.

Ver. 1.21
•	  Added SSID stealth mode setting.
•	  Fixed minor bugs.

Ver. 1.30
•	Added enhanced security (for California Legislation)
o	Discarded the default password to require an access password for product settings.
Ver. 1.41
•	Added a solution to Frag Attacks Wi-Fi vulnerability 
o	Improved the connection stability 
Ver. 1.42
•	Added support for Winbond Flash.
o	Compatible with additional compatible parts
Ver. 1.43

The SX-590 FW will be upgraded from Ver1.42 to Ver1.43 with the following updates:
•	Fix the access point mode communication problem with illegal frames received.
•	Connectivity improvement with stealth APs and WEP set APs.
•	Fix the IEEE802.1X Dynamic WEP communication problem.
•	Wording correction on the configuration web page.